From d87a8072e8129a579246d8d31a591ca2aec05275 Mon Sep 17 00:00:00 2001
From: Tobias Schramm <t.schramm@manjaro.org>
Date: Wed, 4 Mar 2020 22:30:23 +0100
Subject: [PATCH] arm64: dts: rockchip: Add initial support for Pinebook Pro

This commit adds initial dt support for the rk3399 based Pinebook Pro.

Signed-off-by: Tobias Schramm <t.schramm@manjaro.org>
Link: https://lore.kernel.org/r/20200304213023.689983-3-t.schramm@manjaro.org
Signed-off-by: Heiko Stuebner <heiko@sntech.de>

Taken from next-20200313 commit 5a65505a6988443b211d3bf3f5bb5b79907c33b9
---
 arch/arm64/boot/dts/rockchip/Makefile         |    1 +
 .../boot/dts/rockchip/rk3399-pinebook-pro.dts | 1096 +++++++++++++++++
 2 files changed, 1097 insertions(+)
 create mode 100644 arch/arm64/boot/dts/rockchip/rk3399-pinebook-pro.dts

diff --git a/arch/arm64/boot/dts/rockchip/Makefile b/arch/arm64/boot/dts/rockchip/Makefile
index 1f18a9392d15..7de9b61d6415 100644
--- a/arch/arm64/boot/dts/rockchip/Makefile
+++ b/arch/arm64/boot/dts/rockchip/Makefile
@@ -25,6 +25,7 @@ dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3399-nanopc-t4.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3399-nanopi-m4.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3399-nanopi-neo4.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3399-orangepi.dtb
+dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3399-pinebook-pro.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3399-puma-haikou.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3399-roc-pc.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3399-rock-pi-4.dtb
diff --git a/arch/arm64/boot/dts/rockchip/rk3399-pinebook-pro.dts b/arch/arm64/boot/dts/rockchip/rk3399-pinebook-pro.dts
new file mode 100644
index 000000000000..5ea281b55fe2
--- /dev/null
+++ b/arch/arm64/boot/dts/rockchip/rk3399-pinebook-pro.dts
@@ -0,0 +1,1096 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Copyright (c) 2017 Fuzhou Rockchip Electronics Co., Ltd.
+ * Copyright (c) 2018 Akash Gajjar <Akash_Gajjar@mentor.com>
+ * Copyright (c) 2020 Tobias Schramm <t.schramm@manjaro.org>
+ */
+
+/dts-v1/;
+#include <dt-bindings/input/gpio-keys.h>
+#include <dt-bindings/input/linux-event-codes.h>
+#include <dt-bindings/pwm/pwm.h>
+#include <dt-bindings/usb/pd.h>
+#include <dt-bindings/leds/common.h>
+#include "rk3399.dtsi"
+#include "rk3399-opp.dtsi"
+
+/ {
+	model = "Pine64 Pinebook Pro";
+	compatible = "pine64,pinebook-pro", "rockchip,rk3399";
+
+	chosen {
+		stdout-path = "serial2:1500000n8";
+	};
+
+	backlight: edp-backlight {
+		compatible = "pwm-backlight";
+		power-supply = <&vcc_12v>;
+		pwms = <&pwm0 0 740740 0>;
+	};
+
+	edp_panel: edp-panel {
+		compatible = "boe,nv140fhmn49";
+		backlight = <&backlight>;
+		enable-gpios = <&gpio1 RK_PA0 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&panel_en_gpio>;
+		power-supply = <&vcc3v3_panel>;
+
+		ports {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			port@0 {
+				reg = <0>;
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				panel_in_edp: endpoint@0 {
+					reg = <0>;
+					remote-endpoint = <&edp_out_panel>;
+				};
+			};
+		};
+	};
+
+	/*
+	 * Use separate nodes for gpio-keys to allow for selective deactivation
+	 * of wakeup sources via sysfs without disabling the whole key
+	 */
+	gpio-key-lid {
+		compatible = "gpio-keys";
+		pinctrl-names = "default";
+		pinctrl-0 = <&lidbtn_gpio>;
+
+		lid {
+			debounce-interval = <20>;
+			gpios = <&gpio1 RK_PA1 GPIO_ACTIVE_LOW>;
+			label = "Lid";
+			linux,code = <SW_LID>;
+			linux,input-type = <EV_SW>;
+			wakeup-event-action = <EV_ACT_DEASSERTED>;
+			wakeup-source;
+		};
+	};
+
+	gpio-key-power {
+		compatible = "gpio-keys";
+		pinctrl-names = "default";
+		pinctrl-0 = <&pwrbtn_gpio>;
+
+		power {
+			debounce-interval = <20>;
+			gpios = <&gpio0 RK_PA5 GPIO_ACTIVE_LOW>;
+			label = "Power";
+			linux,code = <KEY_POWER>;
+			wakeup-source;
+		};
+	};
+
+	leds {
+		compatible = "gpio-leds";
+		pinctrl-names = "default";
+		pinctrl-0 = <&pwrled_gpio &slpled_gpio>;
+
+		green-led {
+			color = <LED_COLOR_ID_GREEN>;
+			default-state = "on";
+			function = LED_FUNCTION_POWER;
+			gpios = <&gpio0 RK_PB3 GPIO_ACTIVE_HIGH>;
+			label = "green:power";
+		};
+
+		red-led {
+			color = <LED_COLOR_ID_RED>;
+			default-state = "off";
+			function = LED_FUNCTION_STANDBY;
+			gpios = <&gpio0 RK_PA2 GPIO_ACTIVE_HIGH>;
+			label = "red:standby";
+			panic-indicator;
+			retain-state-suspended;
+		};
+	};
+
+	/* Power sequence for SDIO WiFi module */
+	sdio_pwrseq: sdio-pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		clocks = <&rk808 1>;
+		clock-names = "ext_clock";
+		pinctrl-names = "default";
+		pinctrl-0 = <&wifi_enable_h_gpio>;
+		post-power-on-delay-ms = <100>;
+		power-off-delay-us = <500000>;
+
+		/* WL_REG_ON on module */
+		reset-gpios = <&gpio0 RK_PB2 GPIO_ACTIVE_LOW>;
+	};
+
+	/* Audio components */
+	es8316-sound {
+		compatible = "simple-audio-card";
+		pinctrl-names = "default";
+		pinctrl-0 = <&hp_det_gpio>;
+		simple-audio-card,name = "rockchip,es8316-codec";
+		simple-audio-card,format = "i2s";
+		simple-audio-card,mclk-fs = <256>;
+
+		simple-audio-card,widgets =
+			"Microphone", "Mic Jack",
+			"Headphone", "Headphones",
+			"Speaker", "Speaker";
+		simple-audio-card,routing =
+			"MIC1", "Mic Jack",
+			"Headphones", "HPOL",
+			"Headphones", "HPOR",
+			"Speaker Amplifier INL", "HPOL",
+			"Speaker Amplifier INR", "HPOR",
+			"Speaker", "Speaker Amplifier OUTL",
+			"Speaker", "Speaker Amplifier OUTR";
+
+		simple-audio-card,hp-det-gpio = <&gpio0 RK_PB0 GPIO_ACTIVE_LOW>;
+		simple-audio-card,aux-devs = <&speaker_amp>;
+		simple-audio-card,pin-switches = "Speaker";
+
+		simple-audio-card,cpu {
+			sound-dai = <&i2s1>;
+		};
+
+		simple-audio-card,codec {
+			sound-dai = <&es8316>;
+		};
+	};
+
+	speaker_amp: speaker-amplifier {
+		compatible = "simple-audio-amplifier";
+		enable-gpios = <&gpio4 RK_PD3 GPIO_ACTIVE_HIGH>;
+		sound-name-prefix = "Speaker Amplifier";
+		VCC-supply = <&pa_5v>;
+	};
+
+	/* Power tree */
+	/* Root power source */
+	vcc_sysin: vcc-sysin {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc_sysin";
+		regulator-always-on;
+		regulator-boot-on;
+	};
+
+	/* Regulators supplied by vcc_sysin */
+	/* LCD backlight supply */
+	vcc_12v: vcc-12v {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc_12v";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <12000000>;
+		regulator-max-microvolt = <12000000>;
+		vin-supply = <&vcc_sysin>;
+
+		regulator-state-mem {
+			regulator-off-in-suspend;
+		};
+	};
+
+	/* Main 3.3 V supply */
+	vcc3v3_sys: wifi_bat: vcc3v3-sys {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc3v3_sys";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		vin-supply = <&vcc_sysin>;
+
+		regulator-state-mem {
+			regulator-on-in-suspend;
+		};
+	};
+
+	/* 5 V USB power supply */
+	vcc5v0_usb: pa_5v: vcc5v0-usb-regulator {
+		compatible = "regulator-fixed";
+		enable-active-high;
+		gpio = <&gpio1 RK_PB5 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&pwr_5v_gpio>;
+		regulator-name = "vcc5v0_usb";
+		regulator-always-on;
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		vin-supply = <&vcc_sysin>;
+
+		regulator-state-mem {
+			regulator-off-in-suspend;
+		};
+	};
+
+	/* RK3399 logic supply */
+	vdd_log: vdd-log {
+		compatible = "pwm-regulator";
+		pwms = <&pwm2 0 25000 1>;
+		regulator-name = "vdd_log";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <800000>;
+		regulator-max-microvolt = <1400000>;
+		vin-supply = <&vcc_sysin>;
+
+		regulator-state-mem {
+			regulator-on-in-suspend;
+		};
+	};
+
+	/* Regulators supplied by vcc3v3_sys */
+	/* 0.9 V supply, always on */
+	vcc_0v9: vcc-0v9 {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc_0v9";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <900000>;
+		regulator-max-microvolt = <900000>;
+		vin-supply = <&vcc3v3_sys>;
+	};
+
+	/* S3 1.8 V supply, switched by vcc1v8_s3 */
+	vcca1v8_s3: vcc1v8-s3 {
+		compatible = "regulator-fixed";
+		regulator-name = "vcca1v8_s3";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <1800000>;
+		vin-supply = <&vcc3v3_sys>;
+	};
+
+	/* micro SD card power */
+	vcc3v0_sd: vcc3v0-sd {
+		compatible = "regulator-fixed";
+		enable-active-high;
+		gpio = <&gpio0 RK_PA1 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&sdmmc0_pwr_h_gpio>;
+		regulator-name = "vcc3v0_sd";
+		regulator-always-on;
+		regulator-min-microvolt = <3000000>;
+		regulator-max-microvolt = <3000000>;
+		vin-supply = <&vcc3v3_sys>;
+
+		regulator-state-mem {
+			regulator-off-in-suspend;
+		};
+	};
+
+	/* LCD panel power, called VCC3V3_S0 in schematic */
+	vcc3v3_panel: vcc3v3-panel {
+		compatible = "regulator-fixed";
+		enable-active-high;
+		gpio = <&gpio1 RK_PC6 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&lcdvcc_en_gpio>;
+		regulator-name = "vcc3v3_panel";
+		regulator-always-on;
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-enable-ramp-delay = <100000>;
+		vin-supply = <&vcc3v3_sys>;
+
+		regulator-state-mem {
+			regulator-off-in-suspend;
+		};
+	};
+
+	/* M.2 adapter power, switched by vcc1v8_s3 */
+	vcc3v3_ssd: vcc3v3-ssd {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc3v3_ssd";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		vin-supply = <&vcc3v3_sys>;
+	};
+
+	/* Regulators supplied by vcc5v0_usb */
+	/* USB 3 port power supply regulator  */
+	vcc5v0_otg: vcc5v0-otg {
+		compatible = "regulator-fixed";
+		enable-active-high;
+		gpio = <&gpio4 RK_PD2 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&vcc5v0_host_en_gpio>;
+		regulator-name = "vcc5v0_otg";
+		regulator-always-on;
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		vin-supply = <&vcc5v0_usb>;
+
+		regulator-state-mem {
+			regulator-off-in-suspend;
+		};
+	};
+
+	/* Regulators supplied by vcc5v0_usb */
+	/* Type C port power supply regulator */
+	vbus_5vout: vbus_typec: vbus-5vout {
+		compatible = "regulator-fixed";
+		enable-active-high;
+		gpio = <&gpio1 RK_PA3 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&vcc5v0_typec0_en_gpio>;
+		regulator-name = "vbus_5vout";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		vin-supply = <&vcc5v0_usb>;
+
+		regulator-state-mem {
+			regulator-off-in-suspend;
+		};
+	};
+
+	/* Regulators supplied by vcc_1v8 */
+	/* Primary 0.9 V LDO */
+	vcca0v9_s3: vcca0v9-s3 {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc0v9_s3";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		vin-supply = <&vcc_1v8>;
+
+		regulator-state-mem {
+			regulator-on-in-suspend;
+		};
+	};
+
+	mains_charger: dc-charger {
+		compatible = "gpio-charger";
+		charger-type = "mains";
+		gpios = <&gpio4 RK_PD0 GPIO_ACTIVE_LOW>;
+
+		/* Also triggered by USB charger */
+		pinctrl-names = "default";
+		pinctrl-0 = <&dc_det_gpio>;
+	};
+};
+
+&cdn_dp {
+	status = "okay";
+};
+
+&cpu_b0 {
+	cpu-supply = <&vdd_cpu_b>;
+};
+
+&cpu_b1 {
+	cpu-supply = <&vdd_cpu_b>;
+};
+
+&cpu_l0 {
+	cpu-supply = <&vdd_cpu_l>;
+};
+
+&cpu_l1 {
+	cpu-supply = <&vdd_cpu_l>;
+};
+
+&cpu_l2 {
+	cpu-supply = <&vdd_cpu_l>;
+};
+
+&cpu_l3 {
+	cpu-supply = <&vdd_cpu_l>;
+};
+
+&edp {
+	force-hpd;
+	pinctrl-names = "default";
+	pinctrl-0 = <&edp_hpd>;
+	status = "okay";
+
+	ports {
+		edp_out: port@1 {
+			reg = <1>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			edp_out_panel: endpoint@0 {
+				reg = <0>;
+				remote-endpoint = <&panel_in_edp>;
+			};
+		};
+	};
+};
+
+&emmc_phy {
+	status = "okay";
+};
+
+&gpu {
+	mali-supply = <&vdd_gpu>;
+	status = "okay";
+};
+
+&hdmi_sound {
+	status = "okay";
+};
+
+&i2c0 {
+	clock-frequency = <400000>;
+	i2c-scl-falling-time-ns = <4>;
+	i2c-scl-rising-time-ns = <168>;
+	status = "okay";
+
+	rk808: pmic@1b {
+		compatible = "rockchip,rk808";
+		reg = <0x1b>;
+		#clock-cells = <1>;
+		clock-output-names = "xin32k", "rk808-clkout2";
+		interrupt-parent = <&gpio3>;
+		interrupts = <10 IRQ_TYPE_LEVEL_LOW>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&pmic_int_l_gpio>;
+		rockchip,system-power-controller;
+		wakeup-source;
+
+		vcc1-supply = <&vcc_sysin>;
+		vcc2-supply = <&vcc_sysin>;
+		vcc3-supply = <&vcc_sysin>;
+		vcc4-supply = <&vcc_sysin>;
+		vcc6-supply = <&vcc_sysin>;
+		vcc7-supply = <&vcc_sysin>;
+		vcc8-supply = <&vcc3v3_sys>;
+		vcc9-supply = <&vcc_sysin>;
+		vcc10-supply = <&vcc_sysin>;
+		vcc11-supply = <&vcc_sysin>;
+		vcc12-supply = <&vcc3v3_sys>;
+		vcc13-supply = <&vcc_sysin>;
+		vcc14-supply = <&vcc_sysin>;
+
+		regulators {
+			/* rk3399 center logic supply */
+			vdd_center: DCDC_REG1 {
+				regulator-name = "vdd_center";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <750000>;
+				regulator-max-microvolt = <1350000>;
+				regulator-ramp-delay = <6001>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vdd_cpu_l: DCDC_REG2 {
+				regulator-name = "vdd_cpu_l";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <750000>;
+				regulator-max-microvolt = <1350000>;
+				regulator-ramp-delay = <6001>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc_ddr: DCDC_REG3 {
+				regulator-name = "vcc_ddr";
+				regulator-always-on;
+				regulator-boot-on;
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+				};
+			};
+
+			vcc_1v8: vcc_wl: DCDC_REG4 {
+				regulator-name = "vcc_1v8";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1800000>;
+				};
+			};
+
+			/* not used */
+			LDO_REG1 {
+			};
+
+			/* not used */
+			LDO_REG2 {
+			};
+
+			vcc1v8_pmupll: LDO_REG3 {
+				regulator-name = "vcc1v8_pmupll";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1800000>;
+				};
+			};
+
+			vcc_sdio: LDO_REG4 {
+				regulator-name = "vcc_sdio";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <3000000>;
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <3000000>;
+				};
+			};
+
+			vcca3v0_codec: LDO_REG5 {
+				regulator-name = "vcca3v0_codec";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <3000000>;
+				regulator-max-microvolt = <3000000>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc_1v5: LDO_REG6 {
+				regulator-name = "vcc_1v5";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1500000>;
+				regulator-max-microvolt = <1500000>;
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1500000>;
+				};
+			};
+
+			vcca1v8_codec: LDO_REG7 {
+				regulator-name = "vcca1v8_codec";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc_3v0: LDO_REG8 {
+				regulator-name = "vcc_3v0";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <3000000>;
+				regulator-max-microvolt = <3000000>;
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <3000000>;
+				};
+			};
+
+			vcc3v3_s3: SWITCH_REG1 {
+				regulator-name = "vcc3v3_s3";
+				regulator-always-on;
+				regulator-boot-on;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc3v3_s0: SWITCH_REG2 {
+				regulator-name = "vcc3v3_s0";
+				regulator-always-on;
+				regulator-boot-on;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+		};
+	};
+
+	vdd_cpu_b: regulator@40 {
+		compatible = "silergy,syr827";
+		reg = <0x40>;
+		fcs,suspend-voltage-selector = <1>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&vsel1_gpio>;
+		regulator-name = "vdd_cpu_b";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <712500>;
+		regulator-max-microvolt = <1500000>;
+		regulator-ramp-delay = <1000>;
+		vin-supply = <&vcc_1v8>;
+
+		regulator-state-mem {
+			regulator-off-in-suspend;
+		};
+	};
+
+	vdd_gpu: regulator@41 {
+		compatible = "silergy,syr828";
+		reg = <0x41>;
+		fcs,suspend-voltage-selector = <1>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&vsel2_gpio>;
+		regulator-name = "vdd_gpu";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <712500>;
+		regulator-max-microvolt = <1500000>;
+		regulator-ramp-delay = <1000>;
+		vin-supply = <&vcc_1v8>;
+
+		regulator-state-mem {
+			regulator-off-in-suspend;
+		};
+	};
+};
+
+&i2c1 {
+	clock-frequency = <100000>;
+	i2c-scl-falling-time-ns = <4>;
+	i2c-scl-rising-time-ns = <168>;
+	status = "okay";
+
+	es8316: es8316@11 {
+		compatible = "everest,es8316";
+		reg = <0x11>;
+		clocks = <&cru SCLK_I2S_8CH_OUT>;
+		clock-names = "mclk";
+		#sound-dai-cells = <0>;
+	};
+};
+
+&i2c3 {
+	i2c-scl-falling-time-ns = <15>;
+	i2c-scl-rising-time-ns = <450>;
+	status = "okay";
+};
+
+&i2c4 {
+	i2c-scl-falling-time-ns = <20>;
+	i2c-scl-rising-time-ns = <600>;
+	status = "okay";
+
+	fusb0: fusb30x@22 {
+		compatible = "fcs,fusb302";
+		reg = <0x22>;
+		fcs,int_n = <&gpio1 RK_PA2 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&fusb0_int_gpio>;
+		vbus-supply = <&vbus_typec>;
+
+		connector {
+			compatible = "usb-c-connector";
+			data-role = "host";
+			label = "USB-C";
+			op-sink-microwatt = <1000000>;
+			power-role = "dual";
+			sink-pdos =
+				<PDO_FIXED(5000, 2500, PDO_FIXED_USB_COMM)>;
+			source-pdos =
+				<PDO_FIXED(5000, 1400, PDO_FIXED_USB_COMM)>;
+			try-power-role = "sink";
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				port@0 {
+					reg = <0>;
+
+					usbc_hs: endpoint {
+						remote-endpoint =
+							<&u2phy0_typec_hs>;
+					};
+				};
+
+				port@1 {
+					reg = <1>;
+
+					usbc_ss: endpoint {
+						remote-endpoint =
+							<&tcphy0_typec_ss>;
+					};
+				};
+
+				port@2 {
+					reg = <2>;
+
+					usbc_dp: endpoint {
+						remote-endpoint =
+							<&tcphy0_typec_dp>;
+					};
+				};
+			};
+		};
+	};
+};
+
+&i2s1 {
+	#sound-dai-cells = <0>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_8ch_mclk_gpio>, <&i2s1_2ch_bus>;
+	rockchip,capture-channels = <8>;
+	rockchip,playback-channels = <8>;
+	status = "okay";
+};
+
+&io_domains {
+	audio-supply = <&vcc_3v0>;
+	gpio1830-supply = <&vcc_3v0>;
+	sdmmc-supply = <&vcc_sdio>;
+	status = "okay";
+};
+
+&pcie_phy {
+	status = "okay";
+};
+
+&pcie0 {
+	bus-scan-delay-ms = <1000>;
+	ep-gpios = <&gpio2 RK_PD4 GPIO_ACTIVE_HIGH>;
+	max-link-speed = <2>;
+	num-lanes = <4>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&pcie_clkreqn_cpm>;
+	vpcie0v9-supply = <&vcca0v9_s3>;
+	vpcie1v8-supply = <&vcca1v8_s3>;
+	vpcie3v3-supply = <&vcc3v3_ssd>;
+	status = "okay";
+};
+
+&pinctrl {
+	buttons {
+		pwrbtn_gpio: pwrbtn-gpio {
+			rockchip,pins = <0 RK_PA5 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+
+		lidbtn_gpio: lidbtn-gpio {
+			rockchip,pins = <1 RK_PA1 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+
+	dc-charger {
+		dc_det_gpio: dc-det-gpio {
+			rockchip,pins = <4 RK_PD0 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	es8316 {
+		hp_det_gpio: hp-det-gpio {
+			rockchip,pins = <0 RK_PB0 RK_FUNC_GPIO &pcfg_pull_down>;
+		};
+	};
+
+	fusb302x {
+		fusb0_int_gpio: fusb0-int-gpio {
+			rockchip,pins = <1 RK_PA2 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+
+	i2s1 {
+		i2s_8ch_mclk_gpio: i2s-8ch-mclk-gpio {
+			rockchip,pins = <4 RK_PA0 1 &pcfg_pull_none>;
+		};
+	};
+
+	lcd-panel {
+		lcdvcc_en_gpio: lcdvcc-en-gpio {
+			rockchip,pins = <1 RK_PC6 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		panel_en_gpio: panel-en-gpio {
+			rockchip,pins = <1 RK_PA0 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		lcd_panel_reset_gpio: lcd-panel-reset-gpio {
+			rockchip,pins = <4 RK_PD6 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+
+	leds {
+		pwrled_gpio: pwrled_gpio {
+			rockchip,pins = <0 RK_PB3 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		slpled_gpio: slpled_gpio {
+			rockchip,pins = <0 RK_PA2 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	pmic {
+		pmic_int_l_gpio: pmic-int-l-gpio {
+			rockchip,pins = <3 RK_PB2 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+
+		vsel1_gpio: vsel1-gpio {
+			rockchip,pins = <1 RK_PC1 RK_FUNC_GPIO &pcfg_pull_down>;
+		};
+
+		vsel2_gpio: vsel2-gpio {
+			rockchip,pins = <1 RK_PB6 RK_FUNC_GPIO &pcfg_pull_down>;
+		};
+	};
+
+	sdcard {
+		sdmmc0_pwr_h_gpio: sdmmc0-pwr-h-gpio {
+			rockchip,pins = <0 RK_PA1 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+	};
+
+	sdio-pwrseq {
+		wifi_enable_h_gpio: wifi-enable-h-gpio {
+			rockchip,pins = <0 RK_PB2 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	usb-typec {
+		vcc5v0_typec0_en_gpio: vcc5v0-typec0-en-gpio {
+			rockchip,pins = <1 RK_PA3 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+
+	usb2 {
+		pwr_5v_gpio: pwr-5v-gpio {
+			rockchip,pins = <1 RK_PB5 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		vcc5v0_host_en_gpio: vcc5v0-host-en-gpio {
+			rockchip,pins = <4 RK_PD2 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	wireless-bluetooth {
+		bt_wake_gpio: bt-wake-gpio {
+			rockchip,pins = <2 RK_PD3 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		bt_host_wake_gpio: bt-host-wake-gpio {
+			rockchip,pins = <0 RK_PA4 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		bt_reset_gpio: bt-reset-gpio {
+			rockchip,pins = <0 RK_PB1 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+};
+
+&pmu_io_domains {
+	pmu1830-supply = <&vcc_3v0>;
+	status = "okay";
+};
+
+&pwm0 {
+	status = "okay";
+};
+
+&pwm2 {
+	status = "okay";
+};
+
+&saradc {
+	vref-supply = <&vcca1v8_s3>;
+	status = "okay";
+};
+
+&sdmmc {
+	bus-width = <4>;
+	cap-mmc-highspeed;
+	cap-sd-highspeed;
+	cd-gpios = <&gpio0 RK_PA7 GPIO_ACTIVE_LOW>;
+	disable-wp;
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdmmc_clk &sdmmc_cmd &sdmmc_bus4>;
+	sd-uhs-sdr104;
+	vmmc-supply = <&vcc3v0_sd>;
+	vqmmc-supply = <&vcc_sdio>;
+	status = "okay";
+};
+
+&sdio0 {
+	bus-width = <4>;
+	cap-sd-highspeed;
+	cap-sdio-irq;
+	keep-power-in-suspend;
+	mmc-pwrseq = <&sdio_pwrseq>;
+	non-removable;
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdio0_bus4 &sdio0_cmd &sdio0_clk>;
+	sd-uhs-sdr104;
+	status = "okay";
+};
+
+&sdhci {
+	bus-width = <8>;
+	mmc-hs200-1_8v;
+	non-removable;
+	status = "okay";
+};
+
+&spi1 {
+	max-freq = <10000000>;
+	status = "okay";
+
+	spiflash: flash@0 {
+		compatible = "jedec,spi-nor";
+		reg = <0>;
+		m25p,fast-read;
+		spi-max-frequency = <10000000>;
+	};
+};
+
+&tcphy0 {
+	status = "okay";
+};
+
+&tcphy0_dp {
+	port {
+		tcphy0_typec_dp: endpoint {
+			remote-endpoint = <&usbc_dp>;
+		};
+	};
+};
+
+&tcphy0_usb3 {
+	port {
+		tcphy0_typec_ss: endpoint {
+			remote-endpoint = <&usbc_ss>;
+		};
+	};
+};
+
+&tcphy1 {
+	status = "okay";
+};
+
+&tsadc {
+	/* tshut mode 0:CRU 1:GPIO */
+	rockchip,hw-tshut-mode = <1>;
+	/* tshut polarity 0:LOW 1:HIGH */
+	rockchip,hw-tshut-polarity = <1>;
+	status = "okay";
+};
+
+&u2phy0 {
+	status = "okay";
+
+	u2phy0_otg: otg-port {
+		status = "okay";
+	};
+
+	u2phy0_host: host-port {
+		phy-supply = <&vcc5v0_otg>;
+		status = "okay";
+	};
+
+	port {
+		u2phy0_typec_hs: endpoint {
+			remote-endpoint = <&usbc_hs>;
+		};
+	};
+};
+
+&u2phy1 {
+	status = "okay";
+
+	u2phy1_otg: otg-port {
+		status = "okay";
+	};
+
+	u2phy1_host: host-port {
+		phy-supply = <&vcc5v0_otg>;
+		status = "okay";
+	};
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_xfer &uart0_cts &uart0_rts>;
+	uart-has-rtscts;
+	status = "okay";
+
+	bluetooth {
+		compatible = "brcm,bcm4345c5";
+		clocks = <&rk808 1>;
+		clock-names = "lpo";
+		device-wakeup-gpios = <&gpio2 RK_PD3 GPIO_ACTIVE_HIGH>;
+		host-wakeup-gpios = <&gpio0 RK_PA4 GPIO_ACTIVE_HIGH>;
+		max-speed = <1500000>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&bt_host_wake_gpio &bt_wake_gpio &bt_reset_gpio>;
+		shutdown-gpios = <&gpio0 RK_PB1 GPIO_ACTIVE_HIGH>;
+		vbat-supply = <&wifi_bat>;
+		vddio-supply = <&vcc_wl>;
+	};
+};
+
+&uart2 {
+	status = "okay";
+};
+
+&usb_host0_ehci {
+	status = "okay";
+};
+
+&usb_host0_ohci {
+	status = "okay";
+};
+
+&usb_host1_ehci {
+	status = "okay";
+};
+
+&usb_host1_ohci {
+	status = "okay";
+};
+
+&usbdrd3_0 {
+	status = "okay";
+};
+
+&usbdrd_dwc3_0 {
+	dr_mode = "host";
+	status = "okay";
+};
+
+&usbdrd3_1 {
+	status = "okay";
+};
+
+&usbdrd_dwc3_1 {
+	dr_mode = "host";
+	status = "okay";
+};
+
+&vopb {
+	status = "okay";
+};
+
+&vopb_mmu {
+	status = "okay";
+};
+
+&vopl {
+	status = "okay";
+};
+
+&vopl_mmu {
+	status = "okay";
+};
-- 
2.25.1

